Index: DamClients/DamUI/trunk/doc/DAM UI - Functional Design/ResultsDisplay.tex
===================================================================
diff -u -r6509 -r6514
--- DamClients/DamUI/trunk/doc/DAM UI - Functional Design/ResultsDisplay.tex	(.../ResultsDisplay.tex)	(revision 6509)
+++ DamClients/DamUI/trunk/doc/DAM UI - Functional Design/ResultsDisplay.tex	(.../ResultsDisplay.tex)	(revision 6514)
@@ -13,7 +13,7 @@
 An optional graphic presentation of the results must be offered when applicable (e.g.  the picture of the final slip circle for a bishop stability calculation).
 It must also be possible to open/recalculate the individual result in the original program from within \ProgramName when applicable. 
 
-\subsection{Stabilty results}
+\subsection{Stability results}
 The results presented in the table for the stability calculations must be (at least but not limited to):
 \begin{itemize}
 	\item name of the location
@@ -99,12 +99,17 @@
 The data in this file will be used to display the adapted surfaceline graphically when this is available. For this purpose, the file should be read upon selection of the result.
 
 \section{Display results in a graph view}\label{sec:USDisplayResultsGraphic}
-Based on the results of the calculation it should be possible to display the following views per calculated (design and/or subsoil) scenario per location.
+\subsection{Cross section view}
+Based on the results of the calculation it should be possible to display the following items 
+in a cross section view per calculated (design and/or subsoil) scenario per location.
 \begin{itemize}
 	\item The adapted surfaceline when a design calculation has been performed with adaption.
 	\item The resulting slipcircle when a stability calculation has been performed.
 \end{itemize}
 
+\subsection{Time series of safety factors}
+When a Calamity project has been calculated it should be possible to view a chart per location with a time series of the safety factors.
+
 \section{Open individual D-Stability projects}\label{sec:USOpenDStability}
 When a stability calculation has been performed it should be possible to open the stability calculation 
 in D-Stability for each calculated (design and/or subsoil) scenario per location.
