\chapter{RRD scenario selection} \label{sec:RRDScenarioSelection}

For the assessment of regional dikes, \ProgramName must calculate several assessment scenarios (RRD-scenario) depending on:

 \begin{itemize}
	\item the type embankment (peat/other); green block in \autoref{fig:RRDClay} and \autoref{fig:RRDPeat};
	\item the hydraulic shortcut (yes/no); brown block in \autoref{fig:RRDClay}, \autoref{fig:RRDPeat} and in detail in \autoref{fig:HydraulicShortcut};
  \item the uplift situation (yes/no); purple blocks in \autoref{fig:RRDClay} and blue blocks in \autoref{fig:RRDPeat}.
\end{itemize}

This results in a variation of RRD scenarios, summed up in \autoref{tab:RRDScenarios}

\begin{figure}[H]
  \begin{center}
    \includegraphics[width=15cm]{pictures/RRDClay.png}
  \end{center}
  \caption{Flowchart of embankments other than peat}
  \label{fig:RRDClay}
\end{figure}


\begin{figure}[H]
  \begin{center}
    \includegraphics[width=15cm]{pictures/RRDPeat.png}
  \end{center}
  \caption{Flowchart of embankments of peat}
  \label{fig:RRDPeat}
\end{figure}

\begin{figure}[H]
  \begin{center}
    \includegraphics[width=15cm]{pictures/HydraulicShortcut.png}
  \end{center}
  \caption{Flowchart of hydraulic shortcut}
	\label{fig:HydraulicShortcut}
\end{figure}


\begin{table}[H]
\centering
\begin{tabular}{|p{18mm}|p{37mm}|p{20mm}|p{20mm}|p{\textwidth-105mm-36pt}|}
\hline
\textbf{RRD Scenario} & \textbf{Condition} & \textbf{Hydraulic Shortcut} & \textbf{Uplift} & \textbf{Model} \\ \hline
1 & Dry	& yes & yes & Uplift \\ \hline
2 & Dry & no & yes & Uplift \\ \hline
3 & Wet	& yes & yes & Uplift \\ \hline
4 & Wet	& no & yes & Bishop \\ \hline
5 & Dry	& yes & yes & Bishop \\ \hline
6 & Dry & no & yes & Bishop \\ \hline
7 & Wet	& yes & yes & Bishop \\ \hline
8 & Wet	& no & yes & Bishop \\ \hline
9 & Dry	& yes/no & yes & Horizontal equilibrium \\ \hline
10 & Wet & yes/no & yes & Piping \\ \hline
11 & Dry & yes/no & yes & Piping \\ \hline
\end{tabular}
\caption{RRD scenarios}
\label{tab:RRDScenarios}
\end{table}